# FRCS Assumptions:



## Tree Volume

Chip Trees <= 80 ft3

Small Log Trees <= 80 ft3

Large Log Trees > 80 ft3

## Wood Density

For chip trees, small log trees or large log trees, if the wood density is not specified by a user, it is assumed as 50 lb/ft3.

## Hardwood fraction

For chip trees, small log trees or large log trees, if the hardwood fraction is not specified by a user, then it is assumed as 0.

## Logs Per Tree

Logs per chip tree was assumed as 1.